{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["采购救灾物资清单及要求","Sheet3"],"not_rendered":{"images":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"采购救灾物资清单及要求","index":0,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["开平市发展和改革局2024年购置救灾物资参数表"]
["序号","物资种类","单位","要求","备注"]
[1,"棉被","床","1.5m×2m,6公斤以上。填充物：100%聚酯纤维。所有材料要符合 GB18401-2010《国家纺织产品基本安全技术规范》B 类，GB/T22796-2009《被.被套》标准\n要求。","军绿色"]
[2,"军大衣    ","件"," 军绿色。长款，均码，防风防水绸面料、羊绒内胆，所有材料要符合GB18401-2010《国家纺织产品基本安全技术规范》C类，GB/T2664-2017的标准要求。 ","根据采购防寒服数量平均分配码数"]
[3,"毛巾被","张","1.5m×2m；材质：全棉（缎档及装饰部分除外）；安全类别：GB18401-2010(B类）；执行标准：GB/T22864-2009；等级：合格"]
[4,"折叠床","张","1、稳固的钢管床架，床面麻布面料，厚实的棉麻质感，清爽透气，耐脏耐磨兼具保暖透气特性；床面包裹一层海绵，避免木板过硬而降低睡眠的舒适性。含滑轮，方便移动，折叠不占地方。\n2、功能：折叠，四折床。\n3、展开尺寸：190*80*27cm，折叠尺寸：80*33*61cm。\n4、颜色：灰色。\n5、木板床厚度：0.7cm。\n6、海绵垫厚度：0.8cm。\n7、重量：约17kg  承重：100kg。\n8、表面处理：磨砂黑喷漆。"]
[5,"帐篷","顶","1、规格尺寸：3700mm×3200mm×1750mm×2670mm；使用面积12㎡。\n2、符合MZ/T 011.2-2010《救灾帐篷第2部分12㎡单帐篷》检验标准。\n3、帐篷主要材料规格：\n（1）篷体面料：采用颜色为天蓝色PVC涂层布，规格：333dtex×333dtex涤纶丝；\n（2）阻燃性能：续燃时间：经向、纬向≤8s；阴燃时间：经向、纬向≤0s；损毁长度：经向、纬向≤80mm；\n（3）通用杆、地杆、立杆：采用Q235Φ25mm×1.0mm 焊接钢管； 壁厚 1.0mm±0.10mm，喷塑 96h 耐盐雾不起泡、脱落 无锈斑；\n4、帐篷主体按要求印制标识。"]
[6,"折叠一体桌椅","套","桌椅一体、一桌四椅，桌面高强度PP板，高硬度、高韧性，桌子四周为铝合金包边，桌子承重120斤以上，凳子承重100斤以上。"]
[7,"净水机","台","户外使用。产水流量：500L/h,总净水量：20000L；过滤介质：超低压中空纤维膜（过滤精度＜0.2 微米）、聚酯纤维、椰壳活性炭水源类型： I-III 类地表水、地下水；去除物质：泥沙、铁锈、悬浮物、沉淀物、消毒副产物、细菌等物质；使用寿命： 滤芯连续使用不低于 15 天，持续使用需要更换过滤介质；产品主体通风干燥存储 5 年（不含过滤介质）；供电类型：外接电源 AC220V /AC24V；进 水 PH：6~9；工作温度：4℃~40℃；材质：外箱体采用防爆 ABS+铝合金材质；附件：软管、电池、变压器、说明书、TDS 检测笔；产品符合：GB/T 5750.4-2006、GB/T 5750.5-2006、GB/T 5750.12-2006 标准"]
[8,"彩条布","平方米","规格：厚≥120g/㎡；宽度：4米；材质：全新料聚乙烯；说明：加厚耐磨、耐腐蚀、抗酸碱、抗撕裂"]
[9,"防潮垫","张","1.5m×2m；执行标准：GB/4806.92016,GB/15979-2002;等级：合格品。说明：加厚，防水隔潮，附收纳袋。"]
[10,"不锈钢餐具（套装）","套","餐盘、汤碗、筷子、汤勺均304不锈钢，加厚加深，五格分格"]
[11,"牙刷","个","刷毛类型：高密软毛\n适用人群：成人\n刷毛：0.15mm\n规格：4支","4支/包"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}