{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["采购救灾物资清单及要求","Sheet3"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"采购救灾物资清单及要求","index":0,"n_rows":4,"n_cols":5,"rows_kept":4,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["开平市发展和改革局2025年购置救灾物资参数表"]
["序号","物资种类","单位","要求","备注"]
[1,"折叠床","张","1、稳固的钢管床架，床面麻布面料，厚实的棉麻质感，清爽透气，耐脏耐磨兼具保暖透气特性；床面包裹一层海绵，避免木板过硬而降低睡眠的舒适性。含滑轮，方便移动，折叠不占地方。\n2、功能：折叠，四折床。\n3、展开尺寸：190*80*27cm，折叠尺寸：80*33*61cm。\n4、颜色：灰色。\n5、木板床厚度：0.7cm。\n6、海绵垫厚度：0.8cm。\n7、重量：约17kg  承重：100kg。\n8、表面处理：磨砂黑喷漆。"]
[2,"帐篷","顶","1、规格尺寸：3700mm×3200mm×1750mm×2670mm；使用面积12㎡。\n2、符合MZ/T 011.2-2010《救灾帐篷第2部分12㎡单帐篷》检验标准。\n3、帐篷主要材料规格：\n（1）篷体面料：采用颜色为天蓝色PVC涂层布，规格：333dtex×333dtex涤纶丝；\n（2）阻燃性能：续燃时间：经向、纬向≤8s；阴燃时间：经向、纬向≤0s；损毁长度：经向、纬向≤80mm；\n（3）通用杆、地杆、立杆：采用Q235Φ25mm×1.0mm 焊接钢管； 壁厚 1.0mm±0.10mm，喷塑 96h 耐盐雾不起泡、脱落 无锈斑；\n4、帐篷主体按要求印制标识。"]

{"sheet":"Sheet3","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}